July 20, 1995

IBM ThinkPad PCMCIA Features Diskette Version 1.30
==================================================


------------------------------------------------------------------------
GENERAL INFORMATION

This package contains the PCMCIA Features Diskette for the following
ThinkPads:

  340, 340CSE
  350, 350C
  355, 355C, 355CS
  360, 360C, 360CS, 360P, 360CSE, 360CE, 360PE
  370C
  500
  510CS
  701C
  720, 720C
  750, 750C, 750P, 750CS, 750CE
  755C, 755CS, 755CE, 755CD, 755CSE, 755CX, 755CV, 755CDV


If you are experiencing one of the problems listed in the following
Summary of Problem Fixes section, please follow your computer manual
to update the drivers for your ThinkPad 755CD/CE/CSE/CX/CV/CDV.


Summary of New Functions and Problem Fixes
------------------------------------------

        Changed/Fixed Item
        ------------------
        Note: n.nn  Diskette Version (e.g. 1.20  Version 1.20)
              (New) New function or enhancement


========================
PCMCIA Features Diskette
========================

Released Version
----------------

 Version 1.00   Sep. 30 1994   Initial Release
 Version 1.01   Nov. 30 1994   2nd Release for
                                - Corrective Services
 Version 1.20   Feb. 17 1995   3rd Release for
                                - OS/2 Warp Support
                                - Corrective Services
 Version 1.30   Apr. 21 1995   4th Release for
                                - Corrective Services

Changed/Fixed Item
------------------

DOS/Windows

 1.01  IRQ of PCMCIA modem card is not configured as 4(3) even when it
       is configured COM3(COM4).
 1.01  Norton Disk Doctor(NDD) causes "Divide overflow" error.
 1.30  (New) The DOS Card Service driver becomes smaller.
 1.30  Some PCMCIA cards which use the Card Service level mode don't
       work. (The DOS Card Service driver doesn't set IRQ as required
       on the CS 2.1 level mode.)
 1.30  DOS Ethernet connection intermittently fails on long run.

OS2

 1.01  PC Card Director sometimes hangs on OS/2 WARP when it is in ICON
        view.
 1.20  PC Card Director doesn't support the PC Card(s) in IBM Dock II
        (docking station) correctly when "hot-docking".
 1.20  (New) The Card Service supports OS/2 Warp, Resource Manager.
 1.20  2400/9600 PCMCIA Modem (Japan only) can't be enabled.
 1.30  5250J/SDLC-J (Japan only) can't be used under OS2 2.1x (and Warp)
 1.30  The system with the 'PC/3270 for OS/2' installed hangs when
        the multiple 3270 windows are opened then all exit.
 1.30  OS2 Ethernet connection intermittently fails on long run.





*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*
NOTE: 
** NO WARRANTY **  ANY USE BY YOU OF THE SOFTWARE IS AT YOUR OWN RISK.
THE SOFTWARE IS PROVIDED FOR USE "AS IS" WITHOUT WARRANTY OF ANY KIND. 
TO THE MAXIMUM EXTENT PERMITTED BY LAW, IBM AND ITS SUPPLIERS DISCLAIM 
ALL WARRANTIES OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING, WITHOUT
LIMITATION, IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A 
PARTICULAR PURPOSE. IBM IS NOT OBLIGATED TO PROVIDE ANY UPDATES TO THE
SOFTWARE.

NO LIABILITY FOR CONSEQUENTIAL DAMAGES.  In no event shall IBM or its 
suppliers be liable for any damages whatsoever (including, without limitation, 
incidental, direct, indirect special and consequential damages, damages for 
loss of business profits, business interruption, loss of business information, 
or other pecuniary loss) arising out of the use or inability to use this
product, even if IBM has been advised of the possibility of such damages.
*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*
