  The video device driver for ThinkPad 355, 360, 755C/Cs systems is
  included in Windows 95** and it is automatically installed by
  Windows 95 Setup program.  You don't need ThinkPad Windows video
  device driver any longer but still need to install ThinkPad VESA
  video driver. The following procedure enables Windows 95 video
  device driver functions.

  <Enabling Windows 95 Video device driver>
  1. Check your CONFIG.SYS file and look for the following statement.

     :
     DEVICE=C:\IBMVESA\VESA.EXE
     :
     (Note: The directory "C:\IBMVESA" could be different if you
      have installed ThinkPad DOS video device driver into a
      different subdirectory.)

     If you find the statement, your system is already set up for
     Windows 95 video device driver for ThinkPad.  If not, go to
     the next step.
  2. Obtain ThinkPad Video feature diskette.  (The latest version as
     of 6/1/95 is 1.33) and insert it into the diskette drive.
  3. Go to the DOS command prompt.  Then, type A:VINSTALL and press
     Enter.  The supported display list appears.
  4. Using the Arrow keys, highlight the display type which you
     use with your ThinkPad, and press Enter.
  5. Follow the instructions on the screen to save your display
     selection; then press F3 to exit the menu.
  6. Remove the diskette from the diskette drive; then restart the
     system.  The ThinkPad is now ready to work with Windows 95
     video device driver.

  <Verifying Windows 95 device driver setup for ThinkPad 755C/Cs>
  1. After installing or set up Windows 95 on your ThinkPad; click
     "My Computer".
  2. Click "Control Panel"; Click "Display"; Click on "Setting" tab.
  3. Click "Change Display Type..." button.
  4. Make sure that Adapter Type is "Western Digital".
  5. Close "Change Display Type" windows; verify that "256 Color" can
     be selected in "Color palette".

NOTE:
-----
Horizontal stripe appears with mouse pointer on external CRT
When you attach a high resolution external CRT monitor and switch
between a MS-DOS full screen session and Windows 95 desktop, you
may observe a horizontal stripe with the mouse pointer.  If this
happens, take the following steps.

   1. Click "My Computer"
   2. Click "Control Panel"
   3. Click "System"
   4. Click on "Performance" tab
   5. Click "Graphics..." button
   6. Move the slider of "Hardware acceleration" left one notch
   7. You will be prompted to restart the system

   Upon next system boot, the horizontal stripe should disappear.

*  Trademark of IBM Corporation
** Trademark of Microsoft Corporation
