
IBM ThinkPad                                            May 21, 1997
Mwave DSP Features Diskettes for OS/2
Version 2.24
==========================================

What These Diskettes Do
-----------------------
There are three diskettes supporting the Mwave DSP features
for OS/2.

Supported Models
----------------
The following ThinkPad models are equipped with the Mwave features:
    - ThinkPad 755CD, 755CDV, 755CE, 755CSE, 755CV, 755CX
    - ThinkPad 760C, 760CD, 760E, 760ED, 760XD

Summary of Changes
------------------
Where: <n.nn>  Diskette version (for example, 1.00 means Version 1.00)
        (New)  New function or enhancement
        (Fix)  Correction to existing function
        (Restriction)  Remaining restriction
<2.24>
 - (Fix) Faxworks sometimes fails to receive a first fax memo
         in suspend mode when wakeup on ring is used.

<2.22>
 - (Fix) Modems that do not conform to the V.34 specifications
         have poor connectivity.
 - (New) The new "Mwave Quick Tests" application helps isolate
         Mwave problems quickly.
 - (Fix) The board driver has a general protection fault (GPF)
         problem during suspend mode.
 - (Fix) Some wave files of a particular frequency do not run.
 - (Fix) Some class-1 fax-related problems.

 - (Restriction)
        To obtain sound, some games may require
        the SET BLASTER statement, which includes a T3 parameter,
        in the CONFIG.SYS file.

Installation Guide
------------------
Refer to the "INSTALLATION NOTES" in the README.TXT file in the
number-1 diskette of the Mwave DSP Features Diskette for OS/2.

Note: If you are installing the Mwave feature in your
      ThinkPad computer for the first time, you also need to
      install the Mwave DSP Features Diskette for MIDI for OS/2.
      There are six diskettes.

Trademarks
----------
IBM, ThinkPad, Mwave, and OS/2 are trademarks of IBM Corporation.
