                             Patch 1.00

          Patch for Mwave equipped ThinkPads 755 and 760  
          ==============================================

This patch is intended to fix the following problems:
                  
     Wave file buffering as done by Quicktime or Director
     Scan to frame Mpeg or freeze frame problems
     Mpeg lockup
     Mwave modem error when connected to a Java Internet site
     GPF's when playing certain games
     Modem failures connecting to AOL

    
This patch is intended for limited distribution to IBM customers. 
It has received only limited testing before release by IBM, therefore 
it is suggested that any critical data on your hard drive be backed up 
before applying it. This patch will become obsolete with the next 
release of Mwave code.


Patch Scope
===========
This patch is intended for Mwave version 2.25 running under 
Windows 95


Patch Contents
==============
                  
        MPEGA.DSP        30,042  10-24-97 10:35am
        MWSOUND.DRV      50,064  11-03-97 10:42am
        V8.DSP           13,478  09-25-97  2:19pm
        V22.DSP          38,462  10-09-97  2:45pm
        V34.DSP         125,320  10-31-97 11:44am        
        
        Installation Related Files
        ==========================
        INSTALL.EXE        
        INSTALL.MSG         
        INSTALL.DAT         
        README.TXT          

Patch Prerequisites
===================
Mwave version  2.25 must be loaded on your computer running 
under Windows 95 

Patch Instructions  
==================

1. Open Windows DOS box
2. type a:install
3. Install will try to locate all of Mwave.  If everthing is not
   found (probably because you used directory names other than
   the Mwave default ones, or because Mwave exists on another
   drive) it does not matter.  The ONLY directory that has to be
   located is the Mwave Windows Directory (MWW).  If the
   directory found is incorrect, then reply "no" when install
   asks if everthing is correct.  Install will then prompt you
   to type in the correct pathname.
4. Reboot the system for the patch to take effect.

** END OF FILE **
